## Quality Acceptance Inspection Checklist – Lift Equipment

(Subject to modifications when required due to change in requirements)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Purchase Order (PO) #: |  |  | Item Description: |  |
| Vendor Name: |  |  | Location: |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | | **Yes** | **No** | **N/A** |
| Does the lift equipment have a label/identifying mark indicating certification to ANSI B56.10 (Industrial Truck) or ANSI A92 (MEWP)? | |  |  |  |
| If there are any modifications or additions which affect capacity or safe operation, has written approval been received from the manufacturer? | |  |  |  |
| Are there broken welds, missing bolts, or damaged areas on the lift equipment? | |  |  |  |
| Is there leakage or damage on the lift, tilt, and attachment functions of the cylinders? | |  |  |  |
| Are all hydraulic hose connectors threaded on squarely, tightly, and leak-free? | |  |  |  |
| Are the cell caps and terminal covers in place on the battery? | |  |  |  |
| Are all tire lug nuts installed and tightened? | |  |  |  |
| Do all the following features/controls work properly? | |  |  |  |
|  | Gauges |  |  |  |
|  | Steering |  |  |  |
|  | Brakes |  |  |  |
|  | Lights (if equipped) |  |  |  |
|  | Horn |  |  |  |
|  | Back-up Alarm |  |  |  |
|  | Safety Seat (if equipped) |  |  |  |
|  | Windshield Wipers (if equipped) |  |  |  |
|  | Seat Belt (sit down industrial trucks) |  |  |  |
| If equipment has a propane tank: | |  |  |  |
|  | Is the propane tank guard bracket properly positioned and locked down? |  |  |  |
|  | Is the propane hose connector threaded on squarely, tightly, and leak-free? |  |  |  |
|  | | | | |
| *Any nonconformances found during the inspection shall be repaired by the Vendor, at their cost, prior to passing inspection.* | | | | |
|  | | | | |
| Image of ANSI Label | | | | |
|  | | | | |